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Description
For heavy, molten metal riffage, the Jim Root Jazzmaster® V4 delivers crushing detuned tone with a bold new look. We worked closely with the towering Slipknot guitarist to create a brutal-sounding signature Jazzmaster model that complements his heavy playing style - right down to its signature Daemonum™ open-coil EMG® active pickups, shred-worthy 12" radius fingerboard with jumbo frets, sparse control layout and more.
The Jim Root Jazzmaster II dispenses with frivolities such as a vibrato, rhythm circuit, tone control - only crucial essentials remain: a volume control, a 3-way switch and a hardtail bridge, making this guitar a single-purpose weapon of mass destruction. Featuring a mahogany slab body for crushing lows and mids, brilliant Polar White satin finish, maple neck with bound ebony fingerboard and pearloid block inlays, this devastating machine delivers brutal tone with a striking new look.

ITEM SHOWN: Jim Root Jazzmaster® V4, Ebony Fingerboard, Flat White
MODEL #: 0145301780
CASE/GIB BAG: Deluxe Black Tweed Hardshell

Product Specs
Body
Mahogany
Body Finish
Satin Urethane
Body Shape
Jazzmaster®
Bridge
6-Saddle String-Through-Body Hardtail With Block Saddles
Bridge Pickup
EMG® Jim Root Signature Daemonum™ Open-Coil Active Humbucking upgraded to Seymour Duncan Black Winter Humbucker Pickup Set - Blackened
Color
Arctic White
Commodity Code
[object Object]
Configuration
HH
Control Knobs
Black Plastic
Controls
Master Volume
Country Of Origin
Mexico
Dimensions
6.25x17.25x45.25 IN
Fingerboard
Ebony
Fingerboard Radius
12" (305 mm)
Fret Size
Jumbo
Hardware Finish
Black
Model Name
Jim Root Jazzmaster® V4, Ebony Fingerboard, Flat White
Neck Construction
4-Bolt Standard
Neck Finish
Satin Urethane
Neck Finish
Satin Urethane
Neck Material
Maple
Neck Pickup
EMG® Jim Root Signature Daemonum™ Open-Coil Active Humbucking upgraded to Seymour Duncan Black Winter Humbucker Pickup Set - Blackened
Neck Shape
Thin "C"
Number of Frets
22
Nut Material
Synthetic Bone
Nut Width
1.685" (42.8 mm)
Orientation
Right-Hand
Pickguard
None
Pickup Configuration
HH
Pickup Switching
3-Position Blade: Position 1. Bridge Pickup, Position 2. Bridge and Neck Pickups, Position 3. Neck Pickup
Position Inlays
Pearliod Block with Luminlay Fluorescent Side Dots
Refinement Neck Material
Maple
Refinement Neck Shape
C Shape
Scale Length
25.5" (648 mm)
Series
Artist Signature
String Nut
Synthetic Bone
Strings
Fender® USA 250R Nickel Plated Steel (.010-.046 Gauges), PN 0730250406
Tuning Machines
Deluxe Staggered Cast/Sealed Locking
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